|  |  |  |  |
| --- | --- | --- | --- |
| Header 1 | Header 2 | Header 3 |  |
| Instruction 1 |  |  |  |
|  |  |  |  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Results – Day 1** | | | | | | | | |
| **Room No.** | **T**  **ept Point     ID No.** | **ISO Classification** | **Expected Result**  **Non-Viable Particulate**  **(NMT)** | | **Actual Result**  **Non-Viable Particulate** | | **Result Acceptable** | **Verified**  **By/Date** |
| **>0.5** **µm particles / m3** | **>5.0** **µm particles / m3** | **>0.5** **µm particles / m3** | **>5.0** **µm particles / m3** |
| Room No:  e.g. Room 1401 | 1 | ISO 8  (In Operation) | 3,520,000 | 29,000 |  |  | Yes / No | Verifier  E-Signature |
| 2 |  |  | Yes / No | Verifier  E-Signature |
| 3 |  |  | Yes / No | Verifier  E-Signature |
| …. |  |  | Yes / No | Verifier  E-Signature |
| Average |  |  | Yes / No | Verifier  E-Signature |